# Bumpers

A quick reference for bumper rules.

### Numerical Constraints

* 6" on each side of each outside corner.
* Enclosed in the vertical volume that is 0-7 inches above the ground.
* Team numbers must be 4in.
* 20lbs
* Backed by thick and 5 in. tall plywood.
* May not extend > 1in. from frame perimeter
* Must use stacked pair of 2 pool noodles.
* Any gap between backing material and frame:
  + Less than deep or,
  + Not more than 8in. wide